|  |
| --- |
| C:\Users\WWE\Desktop\W W TM.jpg  AN ISO 9001:2015 Certified Company  **INSPECTION CRITERIA FOR RAW MATERIAL** |
| **ITEM CODE:…….. DOC. NO.: IC/RM/Bobbin**  **ITEM NAME: Bobbin EE13X5X5 8P “H”**  **SHEET 01 OF 01 REV. NO.: 00 DT 07.06.19 REVIEWED DATE: 07.06.19** |
| **VISUAL INSPECTION :-**   |  | | --- | | **1.Solderability of pins should be smooth & shiny.** | | **2.No damage,Breakage of any part of bobbin.** | | **3.Pins head should not be visible from winding side.** | | **4.No char ,flashes on bobbin.** | | **5. Pins should be tight.** | | **6. No excess plastic material should cover on pins.** | | **7.functional check with core(fitment Should be Ok).** | |
| **MADE BY CHECKED BY APPROVED BY**  **DATE** |